# Housing and Dining Facilities (HDS) has adopted amendments for all HDS facilities. Confirm applicable standards with Project Representative on a per Project basis.

**Housing and Dining Services takes the following exceptions highlighted in Gray.**

**DIVISION 05 – METALS**

# 05 51 33 – METAL LADDERS

1. Ladders:

7. HDS: All exposed ground level ladders will have a locking cover over the rungs to a height of 8 feet. Lock will be at an accessible height. Padlock provided by owner.

# END OF DIVISION